#MicroXplorer Configuration settings - do not modify
ADC1.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_VREFINT
ADC1.Channel-3\#ChannelRegularConversion=ADC_CHANNEL_15
ADC1.Channel-4\#ChannelRegularConversion=ADC_CHANNEL_10
ADC1.Channel-5\#ChannelRegularConversion=ADC_CHANNEL_TEMPSENSOR_ADC1
ADC1.CommonPathInternal=ADC_CHANNEL_VREFINT|ADC_CHANNEL_TEMPSENSOR_ADC1|null|null
ADC1.ContinuousConvMode=DISABLE
ADC1.DMAContinuousRequests=DISABLE
ADC1.DiscontinuousConvMode=DISABLE
ADC1.EOCSelection=ADC_EOC_SEQ_CONV
ADC1.EnableInjectedConversion=DISABLE
ADC1.EnableRegularConversion=ENABLE
ADC1.ExternalTrigConv=ADC_EXTERNALTRIG_T2_TRGO
ADC1.IPParameters=Resolution,ContinuousConvMode,DMAContinuousRequests,EOCSelection,Overrun,EnableInjectedConversion,OversamplingMode,EnableRegularConversion,Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,OffsetNumber-2\#ChannelRegularConversion,NbrOfConversionFlag,NbrOfConversion,ExternalTrigConv,Rank-3\#ChannelRegularConversion,Channel-3\#ChannelRegularConversion,SamplingTime-3\#ChannelRegularConversion,OffsetNumber-3\#ChannelRegularConversion,Rank-4\#ChannelRegularConversion,Channel-4\#ChannelRegularConversion,SamplingTime-4\#ChannelRegularConversion,OffsetNumber-4\#ChannelRegularConversion,Rank-5\#ChannelRegularConversion,Channel-5\#ChannelRegularConversion,SamplingTime-5\#ChannelRegularConversion,OffsetNumber-5\#ChannelRegularConversion,master,DiscontinuousConvMode,CommonPathInternal
ADC1.NbrOfConversion=4
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-2\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetNumber-3\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetNumber-4\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetNumber-5\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC1.OversamplingMode=DISABLE
ADC1.Rank-2\#ChannelRegularConversion=1
ADC1.Rank-3\#ChannelRegularConversion=2
ADC1.Rank-4\#ChannelRegularConversion=3
ADC1.Rank-5\#ChannelRegularConversion=4
ADC1.Resolution=ADC_RESOLUTION_12B
ADC1.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.SamplingTime-3\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.SamplingTime-4\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.SamplingTime-5\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.master=1
ADC2.Channel-4\#ChannelRegularConversion=ADC_CHANNEL_10
ADC2.ClockPrescaler=ADC_CLOCK_SYNC_PCLK_DIV2
ADC2.CommonPathInternal=null|null|null|null
ADC2.ContinuousConvMode=DISABLE
ADC2.DMAContinuousRequests=DISABLE
ADC2.EOCSelection=ADC_EOC_SINGLE_CONV
ADC2.EnableInjectedConversion=DISABLE
ADC2.EnableRegularConversion=ENABLE
ADC2.ExternalTrigConv=ADC_EXTERNALTRIG_T1_TRGO
ADC2.IPParameters=ClockPrescaler,ContinuousConvMode,DMAContinuousRequests,EOCSelection,EnableInjectedConversion,Rank1_Channel,EnableRegularConversion,Rank-4\#ChannelRegularConversion,Channel-4\#ChannelRegularConversion,SamplingTime-4\#ChannelRegularConversion,OffsetNumber-4\#ChannelRegularConversion,NbrOfConversionFlag,ExternalTrigConv,CommonPathInternal
ADC2.NbrOfConversionFlag=1
ADC2.OffsetNumber-4\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC2.Rank-4\#ChannelRegularConversion=1
ADC2.Rank1_Channel=ADC_CHANNEL_10
ADC2.SamplingTime-4\#ChannelRegularConversion=ADC_SAMPLETIME_6CYCLES_5
BSP_IP_NAME=NUCLEO-G431KB
CAD.formats=
CAD.pinconfig=
CAD.provider=
COMP1.IPParameters=TriggerMode
COMP1.TriggerMode=COMP_TRIGGERMODE_NONE
COMP3.Hysteresis=COMP_HYSTERESIS_NONE
COMP3.IPParameters=TriggerMode,Hysteresis
COMP3.TriggerMode=COMP_TRIGGERMODE_IT_RISING
Dma.ADC1.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.0.EventEnable=DISABLE
Dma.ADC1.0.Instance=DMA1_Channel1
Dma.ADC1.0.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.0.MemInc=DMA_MINC_ENABLE
Dma.ADC1.0.Mode=DMA_NORMAL
Dma.ADC1.0.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.0.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC1.0.Priority=DMA_PRIORITY_LOW
Dma.ADC1.0.RequestNumber=1
Dma.ADC1.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC1.0.SignalID=NONE
Dma.ADC1.0.SyncEnable=DISABLE
Dma.ADC1.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC1.0.SyncRequestNumber=1
Dma.ADC1.0.SyncSignalID=NONE
Dma.ADC2.2.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC2.2.EventEnable=DISABLE
Dma.ADC2.2.Instance=DMA2_Channel1
Dma.ADC2.2.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC2.2.MemInc=DMA_MINC_ENABLE
Dma.ADC2.2.Mode=DMA_NORMAL
Dma.ADC2.2.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC2.2.PeriphInc=DMA_PINC_DISABLE
Dma.ADC2.2.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC2.2.Priority=DMA_PRIORITY_VERY_HIGH
Dma.ADC2.2.RequestNumber=1
Dma.ADC2.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC2.2.SignalID=NONE
Dma.ADC2.2.SyncEnable=DISABLE
Dma.ADC2.2.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC2.2.SyncRequestNumber=1
Dma.ADC2.2.SyncSignalID=NONE
Dma.Request0=ADC1
Dma.Request1=TIM4_CH1
Dma.Request2=ADC2
Dma.Request3=USART2_TX
Dma.RequestsNb=4
Dma.TIM4_CH1.1.Direction=DMA_PERIPH_TO_MEMORY
Dma.TIM4_CH1.1.EventEnable=DISABLE
Dma.TIM4_CH1.1.Instance=DMA1_Channel2
Dma.TIM4_CH1.1.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.TIM4_CH1.1.MemInc=DMA_MINC_ENABLE
Dma.TIM4_CH1.1.Mode=DMA_CIRCULAR
Dma.TIM4_CH1.1.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.TIM4_CH1.1.PeriphInc=DMA_PINC_DISABLE
Dma.TIM4_CH1.1.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.TIM4_CH1.1.Priority=DMA_PRIORITY_LOW
Dma.TIM4_CH1.1.RequestNumber=1
Dma.TIM4_CH1.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.TIM4_CH1.1.SignalID=NONE
Dma.TIM4_CH1.1.SyncEnable=DISABLE
Dma.TIM4_CH1.1.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.TIM4_CH1.1.SyncRequestNumber=1
Dma.TIM4_CH1.1.SyncSignalID=NONE
Dma.USART2_TX.3.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART2_TX.3.EventEnable=DISABLE
Dma.USART2_TX.3.Instance=DMA1_Channel3
Dma.USART2_TX.3.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_TX.3.MemInc=DMA_MINC_ENABLE
Dma.USART2_TX.3.Mode=DMA_NORMAL
Dma.USART2_TX.3.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_TX.3.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_TX.3.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.USART2_TX.3.Priority=DMA_PRIORITY_LOW
Dma.USART2_TX.3.RequestNumber=1
Dma.USART2_TX.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.USART2_TX.3.SignalID=NONE
Dma.USART2_TX.3.SyncEnable=DISABLE
Dma.USART2_TX.3.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.USART2_TX.3.SyncRequestNumber=1
Dma.USART2_TX.3.SyncSignalID=NONE
FDCAN1.CalculateBaudRateNominal=500000
FDCAN1.CalculateTimeBitNominal=2000
FDCAN1.CalculateTimeQuantumNominal=100.0
FDCAN1.ClockDivider=FDCAN_CLOCK_DIV6
FDCAN1.DataPrescaler=1
FDCAN1.DataSyncJumpWidth=9
FDCAN1.DataTimeSeg1=10
FDCAN1.DataTimeSeg2=9
FDCAN1.ExtFiltersNbr=1
FDCAN1.FrameFormat=FDCAN_FRAME_CLASSIC
FDCAN1.IPParameters=NominalTimeSeg1,NominalTimeSeg2,StdFiltersNbr,ExtFiltersNbr,ClockDivider,NominalSyncJumpWidth,FrameFormat,DataTimeSeg1,DataTimeSeg2,DataSyncJumpWidth,NominalPrescaler,CalculateTimeQuantumNominal,CalculateTimeBitNominal,CalculateBaudRateNominal,DataPrescaler
FDCAN1.NominalPrescaler=1
FDCAN1.NominalSyncJumpWidth=1
FDCAN1.NominalTimeSeg1=16
FDCAN1.NominalTimeSeg2=3
FDCAN1.StdFiltersNbr=1
FREERTOS.BinarySemaphores01=ADC1sem,Dynamic,NULL,Available;ADC2sem,Dynamic,NULL,Available;ICsem,Dynamic,NULL,Depleted
FREERTOS.FootprintOK=true
FREERTOS.INCLUDE_vTaskDelayUntil=1
FREERTOS.IPParameters=Tasks01,configUSE_NEWLIB_REENTRANT,FootprintOK,Queues01,BinarySemaphores01,configTOTAL_HEAP_SIZE,INCLUDE_vTaskDelayUntil
FREERTOS.Queues01=CANTxQueue,10,CAN_Frame_t,0,Dynamic,NULL,NULL;WaterTankQueue,16,MSG_STRUCT,0,Dynamic,NULL,NULL
FREERTOS.Tasks01=defaultTask,0,128,StartDefaultTask,Default,NULL,Dynamic,NULL,NULL;CANbusTask,-2,128,vCanBusTask,As external,NULL,Dynamic,NULL,NULL;ADCTask,-1,256,vADCMeasTask,As external,NULL,Dynamic,NULL,NULL;waterTankTask,-1,256,vWaterTankTask,As external,NULL,Dynamic,NULL,NULL;DisdrometerTask,-1,1024,vDisdrometerTask,As external,NULL,Dynamic,NULL,NULL
FREERTOS.configTOTAL_HEAP_SIZE=20000
FREERTOS.configUSE_NEWLIB_REENTRANT=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.CPN=STM32G431KBT6
Mcu.Family=STM32G4
Mcu.IP0=ADC1
Mcu.IP1=ADC2
Mcu.IP10=OPAMP2
Mcu.IP11=RCC
Mcu.IP12=RTC
Mcu.IP13=SYS
Mcu.IP14=TIM1
Mcu.IP15=TIM2
Mcu.IP16=TIM3
Mcu.IP17=TIM4
Mcu.IP18=USART2
Mcu.IP19=NUCLEO-G431KB
Mcu.IP2=COMP1
Mcu.IP3=COMP3
Mcu.IP4=DAC1
Mcu.IP5=DAC3
Mcu.IP6=DMA
Mcu.IP7=FDCAN1
Mcu.IP8=FREERTOS
Mcu.IP9=NVIC
Mcu.IPNb=20
Mcu.Name=STM32G431K(6-8-B)Tx
Mcu.Package=LQFP32
Mcu.Pin0=PF0-OSC_IN
Mcu.Pin1=PF1-OSC_OUT
Mcu.Pin10=PB0
Mcu.Pin11=PA8
Mcu.Pin12=PA10
Mcu.Pin13=PA11
Mcu.Pin14=PA12
Mcu.Pin15=PA13
Mcu.Pin16=PA14
Mcu.Pin17=PB4
Mcu.Pin18=PB5
Mcu.Pin19=PB8-BOOT0
Mcu.Pin2=PA0
Mcu.Pin20=VP_ADC1_TempSens_Input
Mcu.Pin21=VP_ADC1_Vref_Input
Mcu.Pin22=VP_COMP1_VS_DAC1OUT1
Mcu.Pin23=VP_COMP3_VS_DAC3OUT1
Mcu.Pin24=VP_DAC1_VS_DACI1
Mcu.Pin25=VP_DAC3_VS_DACI1
Mcu.Pin26=VP_FREERTOS_VS_CMSIS_V1
Mcu.Pin27=VP_RTC_VS_RTC_Activate
Mcu.Pin28=VP_RTC_VS_RTC_WakeUp_intern
Mcu.Pin29=VP_SYS_VS_tim6
Mcu.Pin3=PA1
Mcu.Pin30=VP_SYS_VS_DBSignals
Mcu.Pin31=VP_TIM1_VS_ControllerModeTrigger
Mcu.Pin32=VP_TIM1_VS_ClockSourceINT
Mcu.Pin33=VP_TIM1_VS_NoETR
Mcu.Pin34=VP_TIM2_VS_ClockSourceINT
Mcu.Pin35=VP_TIM3_VS_ClockSourceINT
Mcu.Pin36=VP_TIM4_VS_ControllerModeReset
Mcu.Pin37=VP_TIM4_VS_ClockSourceINT
Mcu.Pin38=VP_TIM4_VS_ClockSourceITR
Mcu.Pin39=VP_TIM4_VS_NoInput1
Mcu.Pin4=PA2
Mcu.Pin5=PA3
Mcu.Pin6=PA4
Mcu.Pin7=PA5
Mcu.Pin8=PA6
Mcu.Pin9=PA7
Mcu.PinsNb=40
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32G431KBTx
MxCube.Version=6.14.1
MxDb.Version=DB.6.0.141
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.COMP1_2_3_IRQn=true\:5\:0\:true\:false\:true\:true\:false\:true\:true
NVIC.DMA1_Channel1_IRQn=true\:6\:0\:true\:false\:true\:true\:false\:true\:true
NVIC.DMA1_Channel2_IRQn=true\:5\:0\:true\:false\:true\:true\:false\:true\:true
NVIC.DMA1_Channel3_IRQn=true\:5\:0\:true\:false\:true\:true\:false\:true\:true
NVIC.DMA2_Channel1_IRQn=true\:6\:0\:true\:false\:true\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.FDCAN1_IT0_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.FDCAN1_IT1_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.RTC_WKUP_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:true\:false
NVIC.TIM3_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.TIM6_DAC_IRQn=true\:15\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.TimeBase=TIM6_DAC_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.USART2_IRQn=true\:5\:0\:true\:false\:true\:true\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
OPAMP2.IPParameters=PgaGain,PowerMode
OPAMP2.PgaGain=OPAMP_PGA_GAIN_8_OR_MINUS_7
OPAMP2.PowerMode=OPAMP_POWERMODE_HIGHSPEED
PA0.Locked=true
PA0.Mode=INP
PA0.Signal=COMP3_INP
PA1.Mode=INP
PA1.Signal=COMP1_INP
PA10.GPIOParameters=GPIO_Label
PA10.GPIO_Label=BLUE_LED
PA10.Locked=true
PA10.Signal=S_TIM2_CH4
PA11.Mode=FDCAN_Activate
PA11.Signal=FDCAN1_RX
PA12.Mode=FDCAN_Activate
PA12.Signal=FDCAN1_TX
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA2.Locked=true
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.Locked=true
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PA4.Signal=S_TIM3_CH2
PA5.Mode=PGA Connected-INVERTINGINPUT_IO0_BIAS
PA5.Signal=OPAMP2_VINM0
PA6.Mode=PGA Connected-INVERTINGINPUT_IO0_BIAS
PA6.Signal=OPAMP2_VOUT
PA7.Mode=PGA Connected-INVERTINGINPUT_IO0_BIAS
PA7.Signal=OPAMP2_VINP
PA8.Locked=true
PA8.Signal=S_TIM1_CH1
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=ALGEA_SIG
PB0.Mode=IN15-Single-Ended
PB0.Signal=ADC1_IN15
PB4.GPIOParameters=GPIO_Label
PB4.GPIO_Label=DBG
PB4.Locked=true
PB4.Signal=GPIO_Output
PB5.GPIOParameters=GPIO_PuPd,GPIO_Label
PB5.GPIO_Label=WATER_FLOW
PB5.GPIO_PuPd=GPIO_PULLDOWN
PB5.Locked=true
PB5.Signal=GPXTI5
PB8-BOOT0.GPIOParameters=GPIO_Label
PB8-BOOT0.GPIO_Label=LD2
PB8-BOOT0.Locked=true
PB8-BOOT0.Signal=GPIO_Output
PF0-OSC_IN.GPIOParameters=GPIO_Label
PF0-OSC_IN.GPIO_Label=VBUS
PF0-OSC_IN.Locked=true
PF0-OSC_IN.Mode=IN10-Single-Ended
PF0-OSC_IN.Signal=ADC1_IN10
PF1-OSC_OUT.GPIOParameters=GPIO_Label
PF1-OSC_OUT.GPIO_Label=RAIN_SIG
PF1-OSC_OUT.Mode=IN10-Single-Ended
PF1-OSC_OUT.Signal=ADC2_IN10
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerLinker=GCC
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32G431KBTx
ProjectManager.FirmwarePackage=STM32Cube FW_G4 V1.6.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x400
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=NUCLEO_G431KB_WaterTank_I-Spritz_v2e.ioc
ProjectManager.ProjectName=NUCLEO_G431KB_WaterTank_I-Spritz_v2e
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x800
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_FDCAN1_Init-FDCAN1-false-HAL-true,5-MX_TIM2_Init-TIM2-false-HAL-true,6-MX_TIM3_Init-TIM3-false-HAL-true,7-MX_ADC1_Init-ADC1-false-HAL-true,8-MX_USART2_UART_Init-USART2-true-HAL-false,9-MX_DAC3_Init-DAC3-false-HAL-true,10-MX_COMP3_Init-COMP3-false-HAL-true,11-MX_DAC1_Init-DAC1-false-HAL-true,12-MX_ADC2_Init-ADC2-false-HAL-true,13-MX_TIM4_Init-TIM4-false-HAL-true,14-MX_COMP1_Init-COMP1-false-HAL-true,15-MX_OPAMP2_Init-OPAMP2-false-HAL-true,16-MX_RTC_Init-RTC-false-HAL-true,17-MX_TIM1_Init-TIM1-false-HAL-true
RCC.ADC12Freq_Value=120000000
RCC.AHBFreq_Value=120000000
RCC.APB1CLKDivider=RCC_HCLK_DIV2
RCC.APB1Freq_Value=60000000
RCC.APB1TimFreq_Value=120000000
RCC.APB2Freq_Value=120000000
RCC.APB2TimFreq_Value=120000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=120000000
RCC.EXTERNAL_CLOCK_VALUE=12288000
RCC.FCLKCortexFreq_Value=120000000
RCC.FDCANFreq_Value=60000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=120000000
RCC.HSE_VALUE=24000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=60000000
RCC.I2C2Freq_Value=60000000
RCC.I2C3Freq_Value=60000000
RCC.I2SFreq_Value=120000000
RCC.IPParameters=ADC12Freq_Value,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CRSFreq_Value,CortexFreq_Value,EXTERNAL_CLOCK_VALUE,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2SFreq_Value,LPTIM1Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSI_VALUE,MCO1PinFreq_Value,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PWRFreq_Value,RNGFreq_Value,SAI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value
RCC.LPTIM1Freq_Value=60000000
RCC.LPUART1Freq_Value=60000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=16000000
RCC.PLLN=15
RCC.PLLPoutputFreq_Value=120000000
RCC.PLLQoutputFreq_Value=120000000
RCC.PLLRCLKFreq_Value=120000000
RCC.PWRFreq_Value=120000000
RCC.RNGFreq_Value=120000000
RCC.SAI1Freq_Value=120000000
RCC.SYSCLKFreq_VALUE=120000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=170000000
RCC.USART1Freq_Value=120000000
RCC.USART2Freq_Value=60000000
RCC.USART3Freq_Value=170000000
RCC.USBFreq_Value=120000000
RCC.VCOInputFreq_Value=16000000
RCC.VCOOutputFreq_Value=240000000
RTC.IPParameters=WakeUpClock,WakeUpCounter
RTC.WakeUpClock=RTC_WAKEUPCLOCK_CK_SPRE_16BITS
RTC.WakeUpCounter=59
SH.GPXTI5.0=GPIO_EXTI5
SH.GPXTI5.ConfNb=1
SH.S_TIM1_CH1.0=TIM1_CH1,PWM Generation1 CH1
SH.S_TIM1_CH1.ConfNb=1
SH.S_TIM2_CH4.0=TIM2_CH4,PWM Generation4 CH4
SH.S_TIM2_CH4.ConfNb=1
SH.S_TIM3_CH2.0=TIM3_CH2,PWM Generation2 CH2
SH.S_TIM3_CH2.ConfNb=1
TIM1.Channel-PWM\ Generation1\ CH1=TIM_CHANNEL_1
TIM1.IPParameters=Channel-PWM Generation1 CH1,Prescaler,PeriodNoDither,TIM_MasterOutputTrigger,TIM1_ETR_REMAP-TriggerSource_ETR_Remap_TIM1,PulseNoDither_1,OCMode_PWM-PWM Generation1 CH1,OCFastMode_PWM-PWM Generation1 CH1,OCPolarity_1
TIM1.OCFastMode_PWM-PWM\ Generation1\ CH1=TIM_OCFAST_ENABLE
TIM1.OCMode_PWM-PWM\ Generation1\ CH1=TIM_OCMODE_PWM1
TIM1.OCPolarity_1=TIM_OCPOLARITY_LOW
TIM1.PeriodNoDither=100-1
TIM1.Prescaler=120-1
TIM1.PulseNoDither_1=50
TIM1.TIM1_ETR_REMAP-TriggerSource_ETR_Remap_TIM1=TIM_TIM1_ETR_COMP3
TIM1.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM2.Channel-PWM\ Generation4\ CH4=TIM_CHANNEL_4
TIM2.IPParameters=PeriodNoDither,Prescaler,TIM_MasterOutputTrigger,Channel-PWM Generation4 CH4,PulseNoDither_4
TIM2.PeriodNoDither=499
TIM2.Prescaler=159
TIM2.PulseNoDither_4=50
TIM2.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM3.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_DISABLE
TIM3.Channel-PWM\ Generation2\ CH2=TIM_CHANNEL_2
TIM3.IPParameters=Prescaler,PeriodNoDither,AutoReloadPreload,TIM_MasterOutputTrigger,Channel-PWM Generation2 CH2,PulseNoDither_2,TIM_MasterSlaveMode
TIM3.PeriodNoDither=546-1
TIM3.Prescaler=120-1
TIM3.PulseNoDither_2=273
TIM3.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM3.TIM_MasterSlaveMode=TIM_MASTERSLAVEMODE_ENABLE
TIM4.Channel-Input_Capture1_from_TI1_REMAP_TIM4=TIM_CHANNEL_1
TIM4.ICFilter_CH1=2
TIM4.IPParameters=Channel-Input_Capture1_from_TI1_REMAP_TIM4,TIM4_TI1_REMAP-Input_Capture1_from_TI1_REMAP_TIM4,ICFilter_CH1
TIM4.TIM4_TI1_REMAP-Input_Capture1_from_TI1_REMAP_TIM4=TIM_TIM4_TI1_COMP1
USART2.IPParameters=VirtualMode-Asynchronous
USART2.VirtualMode-Asynchronous=VM_ASYNC
VP_ADC1_TempSens_Input.Mode=IN-TempSens
VP_ADC1_TempSens_Input.Signal=ADC1_TempSens_Input
VP_ADC1_Vref_Input.Mode=IN-Vrefint
VP_ADC1_Vref_Input.Signal=ADC1_Vref_Input
VP_COMP1_VS_DAC1OUT1.Mode=INM_DAC1OUT1
VP_COMP1_VS_DAC1OUT1.Signal=COMP1_VS_DAC1OUT1
VP_COMP3_VS_DAC3OUT1.Mode=INM_DAC3OUT1
VP_COMP3_VS_DAC3OUT1.Signal=COMP3_VS_DAC3OUT1
VP_DAC1_VS_DACI1.Mode=DAC_OUT1_Int
VP_DAC1_VS_DACI1.Signal=DAC1_VS_DACI1
VP_DAC3_VS_DACI1.Mode=DAC_OUT1_Int
VP_DAC3_VS_DACI1.Signal=DAC3_VS_DACI1
VP_FREERTOS_VS_CMSIS_V1.Mode=CMSIS_V1
VP_FREERTOS_VS_CMSIS_V1.Signal=FREERTOS_VS_CMSIS_V1
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_RTC_VS_RTC_WakeUp_intern.Mode=WakeUp
VP_RTC_VS_RTC_WakeUp_intern.Signal=RTC_VS_RTC_WakeUp_intern
VP_SYS_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_SYS_VS_DBSignals.Signal=SYS_VS_DBSignals
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
VP_TIM1_VS_ClockSourceINT.Mode=Internal
VP_TIM1_VS_ClockSourceINT.Signal=TIM1_VS_ClockSourceINT
VP_TIM1_VS_ControllerModeTrigger.Mode=Trigger Mode
VP_TIM1_VS_ControllerModeTrigger.Signal=TIM1_VS_ControllerModeTrigger
VP_TIM1_VS_NoETR.Mode=TriggerSource_ETR_Remap_TIM1
VP_TIM1_VS_NoETR.Signal=TIM1_VS_NoETR
VP_TIM2_VS_ClockSourceINT.Mode=Internal
VP_TIM2_VS_ClockSourceINT.Signal=TIM2_VS_ClockSourceINT
VP_TIM3_VS_ClockSourceINT.Mode=Internal
VP_TIM3_VS_ClockSourceINT.Signal=TIM3_VS_ClockSourceINT
VP_TIM4_VS_ClockSourceINT.Mode=Internal
VP_TIM4_VS_ClockSourceINT.Signal=TIM4_VS_ClockSourceINT
VP_TIM4_VS_ClockSourceITR.Mode=TriggerSource_ITR2
VP_TIM4_VS_ClockSourceITR.Signal=TIM4_VS_ClockSourceITR
VP_TIM4_VS_ControllerModeReset.Mode=Reset Mode
VP_TIM4_VS_ControllerModeReset.Signal=TIM4_VS_ControllerModeReset
VP_TIM4_VS_NoInput1.Mode=Input_Capture1_from_TI1_REMAP_TIM4
VP_TIM4_VS_NoInput1.Signal=TIM4_VS_NoInput1
board=NUCLEO-G431KB
boardIOC=true
rtos.0.ip=FREERTOS
isbadioc=false
